|  |  |
| --- | --- |
| 1. | American Public Health Association. 2017. Standard Methods for the Examination of Water and Wastewater, 23rd Edition. Washington, DC. American Public Health Association, American Water Works Association, Water Environment Federation. |
| 2. | National Guidance For The Permitting, Monitoring, and Enforcement of Water Quality-Based Effluent Limitations Set Below Analytical Detection/Quantitation Levels. U.S. Environmental Protection Agency. March 22, 1994. Draft. |
| 3. | Office of the Federal Register. 2012 (or most recent revision). Code of Federal Regulations Title 40, Part 136. Washington, DC. Office of the Federal Register National Archives and Records Administration. |
| 4. | Schmacher, Brian, Plumb, Russell H., Jr., and Fox, Richard. 1994. Great Lakes Dredged Material Testing and Evaluation Manual, Appendix F: Methods for Chemical and Physical Analyses. Las Vegas, NV: Environmental Monitoring Systems Laboratory. U.S. Environmental Protection Agency: Great Lakes National Program Office and U.S. Army Corps of Engineers, North Central Division. |
| 5. | Shoemaker, J. A. And D. R. Tettenhorst. Method 540. Determination of Selected Organic Chemicals in Drinking Water by Solid Phase Extraction and Liquid Chromatography/Tandem Mass Spectrometry (LC/MS/MS). U.S. Environmental Protection Agency, Washington, DC, 2013. |
| 6. | U.S. Environmental Protection Agency. 1996. ICR Microbial Laboratory Manual. Washington, DC, Office of Research and Development. *EPA/600/R-95/178.* |
| 7. | U.S. Environmental Protection Agency. 1983. Methods for the Chemical Analysis of Water and Wastes Washington, DC: U.S. Environmental Protection Agency. *EPA/600/*4-79-020. |
| 8. | U.S. Environmental Protection Agency. 1993. Methods for the Determination of Inorganic Substances in Environmental Samples. Washington, DC: U.S. Environmental Protection Agency. *EPA/600/R-93/100*. |
| 9. | U.S. Environmental Protection Agency. 1991. Methods for the Determination of Metals in Environmental Samples. Washington, DC: U.S. Environmental Protection Agency. *EPA/600/4-91/01*0. |
| 10. | U.S. Environmental Protection Agency. 1994. Methods for the Determination of Metals in Environmental Samples, Supplement I. Washington, DC: U.S. Environmental Protection Agency. *EPA/600/4-94/111*. |
| 11. | U.S. Environmental Protection Agency. 1990. Methods for the Determination of Organic Compounds in Drinking Water, Supplement I. Washington, DC: U.S. Environmental Protection Agency. *EPA/600/4-90/020*. |
| 12. | U.S. Environmental Protection Agency. 1992. Methods for the Determination of Organic Compounds in Drinking Water, Supplement II. Washington, DC: U.S. Environmental Protection Agency. *EPA/600/R-92/129*. |
| 13. | U.S. Environmental Protection Agency. 1995. Methods for the Determination of Organic Compounds in Drinking Water, Supplement III. Washington, DC: U.S. Environmental Protection Agency. *EPA/600/R-95/131*. |
| 14. | U.S. Environmental Protection Agency. 1994. Technical Notes on Drinking Water Methods. Washington, DC: U.S. Environmental Protection Agency, Office of Research and Development. *EPA/600/R-94/173.* |
| 15. | U.S. Environmental Protection Agency. 1994. Test Methods for Evaluating Solid Waste Physical/Chemical Methods, (SW-846) Revision II, Third Edition. Washington, DC: U.S. Environmental Protection Agency. |
| 16. | U.S. Environmental Protection Agency. 1991. Draft Analytical Methods for Determination of Acid Volatile Sulfide (AVS) in Sediment. Washington, DC: U.S. Environmental Protection Agency Office of Water Office of Science and Technology, Health and Ecological Criteria Division, Washington, D.C. *EPA/821/R-91/100*. |
| 17. | U.S. Environmental Protection Agency, 1997, Method 446.0: In Vitro Determination of Chlorophylls a, b, c1 + c2 and Pheopigments in Marine and Freshwater Algae by Visible Spectrometry. Office of Research and Development. |
| 18. | U.S. Environmental Protection Agency. 1994. Method 1613: Tetra- Through Octa- Chlorinated Dioxins and Furans by Isotope Dilution HRGC/HRMS, Revision B. Washington, DC: U.S. Environmental Protection Agency, Office of Water. EPA 821-B-94-005. (Requests for copies: Water Resource Center 202/260-7786 or 202/260-2814). |
| 19. | U.S. Environmental Protection Agency. 1998. Method 1630, Methyl Mercury in Water by Distillation, Aqueous Ethylation. Office of Water. Engineering and Analysis Division (4303). |
| 20. | U.S. Environmental Protection Agency. 1999. Method 1631. Revision B: Mercury in Water by Oxidation, Purge and Trap, and Cold Vapor Atomic Fluorescence Spectrometry. Office of Water (4303). EPA 821-R-95-027. |
| 21. | U.S. Environmental Protection Agency. 1996. Method 1632: Determination of Inorganic Arsenic in Water by Hydride Generation Flame Atomic Absorption. Washington, DC, Office of Water Engineering and Analysis Division (4303). |
| 22. | U.S. Environmental Protection Agency. 1995. Method 1636: Determination of Hexavalent Chromium by Ion Chromatography. Washington, DC, Office of Water Engineering and Analysis Division (4303). EPA 821-R-95-029. |
| 23. | U.S. Environmental Protection Agency. 1995. Method 1637: Determination of Trace Elements in Ambient Waters by Chelation Preconcentration with Graphite Furnace Atomic Absorption. Office of Water (4303). EPA 821-R-95-030. |
| 24. | U.S. Environmental Protection Agency. 1996. Method 1638: Determination of Trace Elements in Ambient Waters by Inductively Coupled Plasma-Mass Spectrometry. Office of Water (4303). EPA 821-R-95-031. |
| 25. | U.S. Environmental Protection Agency. 1995. Method 1639: Determination of Trace Elements in Ambient Waters by Stabilized Temperature Graphite Furnace Atomic Absorption. Office of Water (4303). EPA 821-R-95-032. |
| 26. | U.S. Environmental Protection Agency. 1995. Method 1640: Determination of Trace Elements in Ambient Waters by On-Line Chelation Preconcentration and Inductively Coupled Plasma-Mass Spectrometry. Office of Water (4303). EPA 821-R-95-033. |
| 27. | U.S. Environmental Protection Agency. 1999. Method 1664, Revision A: N-Hexane Extractable Material (HEM; Oil and Grease) and Silica Get Treated N\_Hexane Extractable Material (SGT-HEM; Non-polar Material) by Extraction and Gravimetry Office of Water, Engineering and Analysis Division (4303). |
| 28. | U.S. Environmental Protection Agency. 1996. Method 1668, DRAFT: Toxic PCBs by Isotope Dilution HRGC/HRMS. Washington, DC: U.S. Environmental Protection Agency, Office of Water. |
| 29. | U.S. Environmental Protection Agency. 1998. Method 1677: Available Cyanide by Flow Injection, Ligand Exchange, and Amperometry. Office of Water, Engineering and Analysis Division(4303).. |
| 30. | U.S. Environmental Protection Agency. 1999. Method 1678: Total Cyanide Determination. Office of Water, Engineering and Analysis Division (4303). |
| 31. | U.S. Environmental Protection Agency. 1996. Method 515.3, “Stand Alone Version”, Determination of Chlorinated Acid in Drinking Water by Liquid-Liquid Extraction, Derivatization and Gas Chromatography with Electron Capture Detection, Revision 1.0. |
| 32. | U.S. Environmental Protection Agency. 1997. Method 549.2, Determination of Diquat and Paraquat In Drinking water by Liquid-Solid Extraction and High Performance Liquid Chromatography with Ultraviolet Detection, Revision 1.0. |
| 33. | U.S. Environmental Protection Agency. 1980. Prescribed Procedures for Measurement of Radioactivity in Drinking Water. Washington, DC: U.S. Environmental Protection Agency, EMSL. EPA-600 4-80-032. |
| 34. | Contractor Supplied Methodology. Due the various specialized techniques utilized for these determinations, IDEM/OWQ will evaluate each Contractor’s methodology. |
| 35. | U.S. Geological Survey, 1977, National Handbook of Recommended Methods for Water Data Acquisition, Chapter 3, Sediment. (June 1978 Revision) |
| 36. | American Society for Testing and Materials, 1982, Standard Test Method for Particle-Size Analysis of Soils, D422-63(1998), Philadelphia, Pennsylvania. |
| 37. | American Society for Testing and Materials, 1982, Standard, Standard Test Methods for Specific Gravity of Soil Solids by Water Pycnometer, D854-00, Philadelphia, Pennsylvania. |
| 38. | U.S. Environmental Protection Agency. 2005, Method 535, Measurement of Chloroacetanilide and Other Acetamide Herbicide Degradates in Drinking Water by Solid Phase Extraction and Liquid Chromatography/Tandem Mass Spectrometry (LC/MS/MS), Revision 1.1, U.S. Environmental Protection Agency Office of Water Office of Science and Technology, Health and Ecological Criteria Division, Washington, D.C., EPA/600/R-05/053 |